FINISHING SCHEDULE- EXTERIOR

A. POURED, TILT-UP CONCRETE, STUCCO, BRICK & MASONRY

Flat:

First Coat:
1738 Acrybond (Vinyl Acrylic- Alkyd Modified)
Second Coat:
1840 Superior Exterior Flat
or
1705 Procoat Acrylic Flat Latex
1710 Procrete Exterior/ Interior Masonry Latex
1900 Weather-Master 100% Acrylic Elastomeric
2000 Tex-Crete Smooth & Texured Concrete Finish.

SATIN:

First Coat:
1738 Acrybond (Vinyl Acrylic- Alkyd Modified)
Second Coat:
1845 Super Exterior Low Sheen

SEMI-GLOSS:

First Coat:
1738 Acrybond (Vinyl Acrylic-Alkyd Modified)
Second Coat:
1745 Super Acrysheen S/G (100% Acrylic)
or
1750 Excel Interior/Exterior Semi-Gloss

GLOSS:

First Coat:
1738 Acrybond (Vinyl Acrylic- Alkyd Modified)
Second Coat:
1751 Excel Interior/ Exterior Gloss Latex Enamel

B. SMOOTHWOOD- DOORS, TRIM AND SIDING

Flat:

First Coat:
1736 Excel Primer (100% Acrylic)
or
UH2772 (Alkyd Primer)
Second Coat:
1740 Excel Acryluxe Flat (100% Acrylic)
or
1840 Super Exterior Flat

Satin:

First Coat:
1736 Excel Primer (100% Acrylic)
or
UH2772 (Alkyd Primer)
Second Coat:
1845 Super Exterior Low Sheen

Semi-Gloss

First Coat:
1736 Excel Primer (100% Acrylic Primer)
or 
UH2772 (Alkyd Primer)
Second Coat:
1745 Super Acrysheen (100% Acrylic)
or
1750 Excel Semi-Gloss (100% Acrylic)

Gloss:

First Coat  
1736 Excel Primer (100% Acrylic)
or
UH2772 (Alkyd Primer)
Second Coat  
1751 Excel Gloss Latex (100% Acrylic)
or
Tech-Gard Alkyd Gloss Enamel

C. ROUGH-SAWN WOOD, SIDING AND TRIM

Flat:

First Coat  
1736 Excel Primer (100% Acrylic)
or
UH2772 (Alkyd Primer)
Second Coat  
1740 Excel Acryluxe Flat (100% Acrylic)
or
1840 Super Exterior Flat

Satin:

First Coat  
1736 Excel Primer (100% Acrylic)
or
UH2772 (Alkyd Primer)
Second Coat  
1845 Super Exterior Low Sheen

Semi-Gloss:

First Coat  
1736 Excel Primer (100% Acrylic)
or
UH2772 (Alkyd Primer)
Second Coat 
1745 Super Acrysheen (100% Acrylic)
or

1750 Excel Semi-Gloss (100% Acrylic)

Gloss:

First Coat
1736 Excel Primer (100% Acrylic)
or
UH2772 (Alkyd Primer)
Second Coat  
1751 Excel Gloss Latex (100% Acrylic)
or
Tech-Gard Alkyd Gloss Enamel

D. WOOD SHINGLES, SHAKES, BEAMS, SIDING:

Semi-Transparent (Waterborne)

First Coat  
1700 Acrylic Stain (Acrylic/ Oil Modified)
Second Coat  
1700 Acrylic Stain (Acrylic/ Oil Modified)

Semi-Transparent (Oil Stain)

First Coat  
Armstrong Weather-Shield

E. HARDBOARD, PARTICLE BOARD AND CHIPBOARD

Flat:

First Coat  
1736 Excel Primer (100% Acrylic)
or
UH2772 (Alkyd Primer)
Second Coat  
1740 Excel Acryluxe Flat (100% Acrylic)
or
1840 Super Exterior Flat

Satin:

First Coat  
1736 Excel Primer (100% Acrylic)
or
UH2772 (Alkyd Primer)
Second Coat  
1845 Super Exterior Low Sheen

Semi-Gloss:

First Coat  
1736 Excel Primer (100% Acrylic)
or
UH2772 (Alkyd Primer)
Second Coat  
1745 Super Acrysheen (100% Acrylic) 
or
1750 Excel Semi-Gloss (100% Acrylic)

Gloss:

First Coat  
1736 Excel Primer (100% Acrylic)
or
UH2772 (Alkyd Primer)
Second Coat.  
1751 Excel Gloss Latex (100% Acrylic)
or
Tech-Gard Alkyd Gloss Enamel

F. GALVANIZED METAL AND ALUMINUM

Flat:

Pretreatment  Ecoprime (Wash)

First Coat 
Galva- Grip (Primer)
Second Coat  
1740 Excel Acryluxe Flat (100% Acrylic)

Satin:

Pretreatment  Ecoprime (Wash)

First Coat  
Galva- Grip (Primer)
Second Coat  
1845 Super Exterior Low Sheen

Semi-Gloss:

Pretreatment  Ecoprime (Wash)

First Coat  
Galva- Grip (Primer)
Second Coat  
1745 Super Acrysheen (100% Acrylic)
or
1750 Excel Semi-Gloss (100% Acrylic)

Gloss:

Pretreatment  Ecoprime (Wash)

First Coat  
Galva- Grip (Primer)
Second Coat  
1751 Excel Gloss (100% Acrylic)
or
Tech-Gard Industrial Gloss Enamel (Alkyd)

G. FERROUS METAL (IRON & STEEL):

Flat:

First Coat  
E-155 Red Oxide Metal Primer (Alkyd)
Second Coat  
1740 Excel Acryluxe Flat (100% Acrylic)
Third Coat  
1740 Excel Acryluxe Flat (100% Acrylic)

Satin:

First Coat  
E-155 Red Oxide Metal Primer (Alkyd)
Second Coat  
1845 Super Exterior Low Sheen
Third Coat  
1845 Super Exterior Low Sheen

Semi-Gloss:

First Coat 
E-155 Red Oxide Metal Primer (Alkyd)
Second Coat  
1745 Super Acrysheen (100% Acrylic)
Third Coat  
1745 Super Acrysheen (100% Acrylic)
or
Second Coat  
1750 Excel Semi-Gloss
Third Coat  
1750 Excel Semi-Gloss

Gloss:

First Coat  
E-155 Red Oxide Metal Primer (Alkyd)
Second Coat  
1751 Excel Gloss (100% Acrylic)
Third Coat  
1751 Excel Gloss (100% Acrylic)
or
Second Coat  
Tech-Gard Industrial Enamel (Alkyd)
Third Coat  
Tech Gard Industrial Enamel (Alkyd)

END OF EXTERIOR PAINTING SECTION